**SAS 500 / 550 se­mi-cou­pler bar with turn­buck­le**  
  
Rein­for­cing cou­pling sys­tem to con­nect bars of the sa­me dia­me­ter, if the con­nec­ting bar is not ro­ta­table and not lon­gi­tu­di­nal­ly ad­jus­ta­ble  
  
Con­sis­ting of:  
1 turn­buck­le (T3105), 1 lock nut (T2003), 1 saw tip,   
1 end cap (T5025 SP), 1x lo­cking/screwing  
SAS 500 / 550 sys­tem ac­cor­ding to ap­pro­val no. Z-1.1-58, Z-1.5-174, Z-1.1-106, Z-1.5-173. Ma­nu­fac­tu­rer: Stahl­werk Anna­hütte, D-83404 Ham­merau  
In­stal­la­ti­on as spe­ci­fied by the struc­tu­ral en­gi­neer.  
  
Dia­me­ter of the rein­force­ment: \_\_\_\_\_\_\_mm