**SAS 500 / 550 end an­cho­r­a­ge with an­chor pla­te and an­chor nut**  
  
Screwed cou­pler sys­tem as rein­for­cing con­nec­tion  
  
Con­sis­ting of:  
1 an­chor pla­te, strai­ght (T2139), 1 an­chor nut (T2002), 1 lock nut,   
short (T2040), 1 saw cut, 1 x lo­cking/screwing  
SAS 500 / 550 sys­tem ac­cor­ding to ap­pro­val no. Z-1.1-58, Z-1.5-174, Z-1.1-106, Z-1.5-173. Ma­nu­fac­tu­rer: Stahl­werk Anna­hütte, D-83404 Ham­merau  
In­stal­la­ti­on as spe­ci­fied by the struc­tu­ral en­gi­neer.  
  
Dia­me­ter of the rein­force­ment: \_\_\_\_\_\_\_mm