**SAS 500 / 550 (BSt 500 S) thre­ad bar sys­tem**  
  
Ac­cor­ding to ap­pro­val no. Z-1.1-58 and Z-1.1-106  
  
Rein­for­cing thre­ad bar cou­pling sys­tem   
Ma­nu­fac­tu­rer: Stahl­werk Anna­hütte, D-83404 Ham­merau  
In­stal­la­ti­on and lengths as spe­ci­fied by the struc­tu­ral en­gi­neer.  
  
Dia­me­ter of the rein­force­ment: from \_\_\_\_\_\_\_ to \_\_\_\_\_\_\_mm